NUCL 402 HMWK 6

1. Percent Pump Power to Plant Power
2. Minimum CPR for typical BWR at 100% power.
3. Pumping Power for typical PWR coolant system.
4. Energy Generated after Shutdown
   1. 1 hour
   2. 1 day
   3. 1 month
   4. 1 year